High level IPC testing

# Large parameters

Verify that all TB parameters can be written to the device, notably the longer ones

* Custom characterization   
  CUSTOM\_CHAR\_POINTS  
  CUSTOM\_CHAR.NUMBER\_OF\_POINTS  
  then CHAR\_SELECTION.TYPE\_1=”Activate Custom”
* PST configuration  
  PST\_CONFIG

# Parameters consistency

Verify that parameters seen in TB match those seen via SA HART commands

* COMPLETE\_STATUS vs command 136