Use of TB parameters

The obvious requirement is that FFP object is populated before use.

## Release 3 items

Project TFS path: $/Firmware-SVI II AP FF/FD-SW

Project changeset version: 58550

Starting point: Search for TB parameters on RHS and also Read handler of PTB. Those owned by APP must ensure that they are populated before use.

NOTE: Used on RHS without pre-populating are extremely hard to test because the act of reading may APPARENTLY fix the problem.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Containing file | | FD-SW/ target\appl\fdev\src\ctrl\_param\_set.c | Review Date | Reviewer |
| Function or data | |  | 16-07-19 |  |
|  | | | | |
| TFS wit |  |  | | |
| Impact | |  | | |
| Additional | |  | | |
| Resolution | |  | | |